

**RELEASE NOTES**

Product: **FW for MI 3365 HW1.0/HD1.0**

Version: **1.0.12.b0fb6e2c**

Release date: **31.01.2024**

**DESCRIPTION OF THE RELEASED PRODUCT:**

FW for MI 3365 OmegaEE XD \_ Series

**Description of changes, dependences and history:**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | MI 3365 | | | | | PC SW | *Minimal FW version of related instruments* | *Changed parameters of AutoSequences (Yes/No)* |
| *#* | *FW version* | *Release date* | *Description of changes:* | *HW / HD version* | *Metrel*  *User Manual version* | ***M****etrel* ***E****lectrical* ***S****afety* ***M****anager*  *version* |
| 3 | 1.0.12.b0fb6e2c | 31.01.2024 | * Updated translations. | HW1.0/HD1.0 | Ver.1.2.2 | Fully supported  V.1.22.0.xxxx | A 1322 (FW:1.32)  A 1422 (FW:1.52)  A 1632 (FW:1.2.16) | / |
| 2 | 1.0.10.ce351659 | 21.11.2023 | * Changed pre-test (check of relays), * Bug fix (changed captions of RCD, PRCD, EV-RCD measurements), * (FWA-130). | HW1.0/HD1.0 | Ver.1.1.1 | Fully supported  V.1.22.0.xxxx | A 1322 (FW:1.27)  A 1422 (FW:1.45)  A 1632 (FW:1.2.16) | / |
| 1 | 1.0.8.a383e469 | 07.11.2023 | * First official FW release. | HW1.0/HD1.0 | Ver.1.1.1 | Fully supported  V.1.22.0.xxxx | A 1322 (FW:1.27)  A 1422 (FW:1.45)  A 1632 (FW:1.2.16) | / |

**INSTALLATION PROCEDURE:**

The instrument can be upgraded from a PC via the RS232 or USB communication port. This enables to keep the instrument up to date even if the standards or regulations change. The firmware upgrade requires internet access and can be carried out from the ***Metrel ES Manager*** software with a help of special upgrading software – ***FlashMe*** which will guide you through the upgrading procedure. For more information refer to **Metrel ES Manager** Help file.

**COMPANY DATA:**

METREL d.o.o

Measuring and Regulation Equipment Manufacturer

Ljubljanska 77

SI-1354 Horjul

Tel: + 386 (0)1 75 58 200

Fax: + 386 (0)1 75 49 226

E-mail: metrel@metrel.si

http://www.metrel.si